Pi Pico

Adafruit moisture sensor:

GPIO0: White (SDA)

GPIO1: Green (SCL)

-\*\*\*Might need to swap?

Relay:

-IN -> GPIO15 Pico: Relay signal for water pump

-VIN -> Pico 3.3V out

-GND -> Pico GND

-COM: PSU GND

-NC: Pump negative terminal

Pump:

-Positive terminal: PSU Input\*\*\*\*